{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M9"]
[]
[]
[]
[]
["","","","","","2AMXM40M4V1B9","2AMXM50M4V1B9"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","552"]
["","","","Ширина","мм","852","852"]
["","","","Глубина","мм","350","350"]
["Масса","Блок","","","кг","36","41"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","500","500"]
["","","Нагревание","Самый низкий","об/мин","320","500"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15"]
["","","","Макс.","°CWB","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","46"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","48"]
["Хладагент","Тип","","","","R-32","R-32"]
["","Заправка","","","кг","0.88","1.15"]
["","Заправка","","","tCO2Eq","0.60","0.78"]
["","ПГП","","","","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20 (1)","20 (1)"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15"]
["","","IU - IU","Макс.","м","7.5","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","30","30"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-230-240","220-230-240"]
["Примечания","","","","","(1) - Для одного помещения","(1) - Для одного помещения"]
["Размеры","Блок","","Высота","мм","","552"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","","48"]
["","Hагрев","","Выс.","дБA","","50"]
["Стандартные аксессуары","Reducer assembly","","","","","1"]