{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 2MXM-M9"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 2MXM50M2V1B9"]
["Холодопроизводительность","Ном.","","кВт","3.0"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","310"]
["","EER","","","4.84"]
["","COP","","","4.58"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A"]
["","","Нагрев","","A"]
["Теплопроизводительность","Мин.","","кВт","4.00"]
["Примечания","","","","(1) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C ст,19°С влт,температура наружного воздуха: 35°C cт, эквивалентная длина трубы с хладагентом: 5м, перепад высот: 0м. Данные для серии со стандартной эффективностью.Используются допуски Eurovent 2015"]
["","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]