{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":23,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FBQ100D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG71L9V1B","FBQ71D2VEB / RZQG71L9V1B (Предварительные данные)","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ100D2VEB / RZQG100L9V1B","FBQ140D2VEB / RZQG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG100L9V1B","FBQ125D2VEB / RZQG125L9V1B (Предварительные данные)","FBQ140D2VEB / RZQG125L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG125L9V1B","FBQ60D2VEB / FBQ60D2VEB / RZQG125L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG125L9V1B","FBQ140D2VEB / RZQG140L9V1B"]
["Холодопроизводительность","Ном.","","кВт","","","","","6.8","","9.5 (2)","","","","","","12.0","","","","","","13.4 (2)"]
["Охлаждение помещений","SEER","","","6.16","5.10","5.10","5.10","6.16","5.10","5.87","5.87","5.10","5.10","5.10","5.10","5.83","6.11","5.10","5.10","5.10","5.10"]
["","Годовое потребление энергии","","кВтч/г","386","466","466","466","386","652","566","566","652","652","652","652","720","687","824","824","824","824"]
["","Производительность","Pрасч.","кВт","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Класс энергоэффективности","","","A++","A","A","A","A++","A","A+","A+","A","A","A","A","A+","A++","A","A","A","A"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","6.00","6.00","6.00","6.00","6.00","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.70","12.70","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","4.31","3.80","3.80","3.80","4.35","3.80","4.78","4.78","3.80","3.80","3.80","3.80","4.37","4.28","3.80","3.80","3.80","3.80"]
["","Класс энергоэффективности","","","A+","A","A","A","A+","A","A++","A++","A","A","A","A","A+","A+","A","A","A","A"]
["","Годовое потребление энергии","","кВтч/г","1,949","2,210","2,210","2,210","1,931","4,163","3,310","3,310","4,163","4,163","4,163","4,163","4,069","4,154","4,683","4,683","4,683","4,683"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","","","","","963","","1,247","","","","","","1,567"]
["","EER","","","","","","","3.53","","3.81 (1)","","","","","","3.83","","","","","","3.35 (1)"]
["","COP","","","","","","","3.96","","4.41 (1)","","","","","","3.83","","","","","","3.60 (1)"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","","","A","","A","","","","","","A"]
["","","Нагрев","","","","","","A","","A","","","","","","A"]
["Теплопроизводительность","Ном.","","кВт","","","","","7.5","","10.80 (2)","","","","","","13.5","","","","","","15.50 (2)"]
["Примечания","","","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]
["","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]