{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":21,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQG71L9V1B","FCQG100FVEB / RZQG71L9V1B","FCQG71FVEB / RZQG71L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG100FVEB / RZQG100L9V1B","FCQG140FVEB / RZQG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG100L9V1B","FCQG60FVEB / FCQG60FVEB / RZQG125L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG125L9V1B","FCQG125FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG125L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG140L9V1B"]
["Холодопроизводительность","Ном.","","кВт","","","6.8","","9.5","","","","","","","","12.0","","","","13.4"]
["Охлаждение помещений","SEER","","","5.10","6.80","6.72","5.10","6.80","6.80","5.10","5.10","5.10","5.10","5.10","5.10","6.00","6.00","5.10","5.10"]
["","Годовое потребление энергии","","кВтч/г","467","350","355","652","489","489","652","652","652","652","824","824","700","700","824","824"]
["","Производительность","Pрасч.","кВт","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Класс энергоэффективности","","","B","A++","A++","B","A++","A++","B","B","B","B","B","B","A+","A+","B","B"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","6.00","6.33","6.33","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.71","12.71","12.66","12.66","12.71","12.71"]
["","SCOP/A","","","3.80","4.20","4.20","3.80","4.61","4.61","3.80","3.80","3.80","3.80","3.80","3.80","4.10","4.10","3.80","3.80"]
["","Класс энергоэффективности","","","A","A+","A+","A","A++","A++","A","A","A","A","A","A","A+","A+","A","A"]
["","Годовое потребление энергии","","кВтч/г","2,211","2,110","2,110","4,164","3,432","3,432","4,164","4,164","4,164","4,164","4,683","4,683","4,323","4,323","4,683","4,683"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","","","1,005","","1,225","","","","","","","","1,610"]
["","EER","","","","","3.39","","3.87","","","","","","","","3.73","","","","3.21"]
["","COP","","","","","3.97","","4.15","","","","","","","","3.63","","","","3.61"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","A","","A","","","","","","","","A"]
["","","Нагрев","","","","A","","A","","","","","","","","A"]
["Теплопроизводительность","Ном.","","кВт","","","7.5","","10.8","","","","","","","","13.5","","","","15.5"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","","","(1) - Годовое потребление энергии соответствует Европейской директиве о маркировке 2002/31/EC","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","","","(2) - SEER и SCOP соответствуют EN 14825","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","","","","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]