{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS60F2VEB / FDXS60F2VEB / RZQG125L8Y1B"]
["Охлаждение помещений","SEER","","","4.80","4.8","5.10"]
["","Годовое потребление энергии","","кВтч/г","496","496","652"]
["","Производительность","Pрасч.","кВт","6.80","6.8","9.50"]
["","Класс энергоэффективности","","","B","B","B"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","6.00","6","10.74"]
["","SCOP/A","","","3.80","3.8","3.80"]
["","Класс энергоэффективности","","","A","A","A"]
["","Годовое потребление энергии","","кВтч/г","2,211","2,211","3,957"]
["Примечания","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["Охлаждение помещений","Класс энергоэффективности","","","","","","B","B"]
["","Производительность","Pрасч.","кВт","","","","9.5","12"]
["","SEER","","","","","","5.1","5.1"]
["","Годовое потребление энергии","","кВтч/г","","","","652","824"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","","","","A","A"]
["","Производительность","Pрасч.","кВт","","","","10.74","12.71"]
["","SCOP/A","","","","","","3.8","3.8"]
["","Годовое потребление энергии","","кВтч/г","","","","3957","4683"]
["Диапазон энергоэффективности","","","","","","","A+++ ~ D","A+++ ~ D"]