{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXS-L"]
[]
[]
[]
[]
["","","","","FHA50AVEB / RXS50L2V1B","FHA60AVEB / RXS60L2V1B"]
["Наружный блок","","","","RXS50L2V1B","RXS60L2V1B"]
["Холодопроизводительность","Ном.","","кВт","5.00","5.70"]
["Теплопроизводительность","Ном.","","кВт","6.00","7.20"]
["Номинальная эффективность","EER","","","3.27","3.31"]
["","COP","","","3.35","3.32"]
["","Годовое потребление энергии","","кВтч","765","861"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","C","C"]
["Охлаждение помещений","Класс энергоэффективности","","","A+","A+"]
["","Производительность","Pрасч.","кВт","5.00","5.70"]
["","SEER","","","5.87","6.02"]
["","Годовое потребление энергии","","кВтч/г","298","332"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A","A"]
["","Производительность","Pрасч.","кВт","4.35","4.71"]
["","SCOP/A","","","3.86","3.87"]
["","Pdh Теплопроизводительность при -10°","","кВт","3.85","4.08"]
["","Годовое потребление энергии","","кВтч/г","1578","1705"]