{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 5MXM-A8"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM20N2V1B / FTXM50N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM35N2V1B / FTXM35N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM71N2V1B / 5MXM90A2V1B8","FTXM42N2V1B / FTXM50N2V1B / 5MXM90A2V1B8","FTXM25N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90A2V1B8"]
["Холодопроизводительность","Ном.","","кВт","7.80","8.00","8.00","8.00","8.00","8.00","8.00"]
["Теплопроизводительность","Ном.","","кВт","10.00","10.00","10.00","10.00","10.00","10.00","10.00"]
["Номинальная эффективность","EER","","","4.15","3.82","3.71","3.73","3.33","3.34","3.72"]
["","COP","","","4.58","4.28","4.08","3.99","3.69","3.74","4.09"]
["","Годовое потребление энергии","","кВтч","940","1047","1077","1073","1202","1199","1075"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","A","A","A"]
["","","Нагрев","","A","A","A","A","A","A","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A++","A++","A++","A++","A++","A++","A++"]
["","Производительность","Pрасч.","кВт","7.80","8.00","8.00","8.00","8.00","8.00","8.00"]
["","SEER","","","7.55","7.29","7.17","7.18","6.84","6.85","7.18"]
["","Годовое потребление энергии","","кВтч/г","366","387","391","392","410","411","391"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A+","A+","A+","A+","A+","A+","A+"]
["","Производительность","Pрасч.","кВт","6.46","6.46","5.60","6.46","4.50","5.20","5.60"]
["","SCOP/A","","","4.50","4.34","4.35","4.20","4.26","4.21","4.36"]
["","Pdh Теплопроизводительность при -10°","","кВт","5.02","4.98","4.47","4.97","3.84","4.19","4.48"]
["","Годовое потребление энергии","","кВтч/г","2010","2083","1803","2152","1478","1731","1799"]