{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Тип","","","","","Воздухоочиститель"]
["Применение","","","","","Напольный тип"]
["Корпус","Цвет","","","","Белый"]
["Размеры","Блок","","Высота","мм","500"]
["","","","Ширина","мм","270"]
["","","","Глубина","мм","270"]
["Вес","Блок","","","кг","6.8"]
["Обслуживаемая площадь","м²","","","","41 (1), 82 (2)"]
["CADR","м³/ч","","","","320"]
["Режим очистки воздуха","Входная мощность","","Turbo","кВт","0.037"]
["","","","M","кВт","0.015"]
["","","","L","кВт","0.010"]
["","","","Бесшумный","кВт","0.008"]
["Уровень звукового давления","Режим очистки воздуха","","Turbo","дБA","53"]
["","","","Средн.","дБA","39"]
["","","","Низк.","дБA","29"]
["","","","Бесшумный","дБA","19"]
["Вентилятор","Расход воздуха","Режим очистки воздуха","Turbo","м³/ч","330"]
["","","","Средний уровень","м³/ч","192"]
["","","","Низк.","м³/ч","120"]
["","","","Бесшумный","м³/ч","66"]
["Способ пылеудаления","","","","","Электростатический HEPA-фильтр"]
["Способ дезодорирования","","","","","Стримерный разряд + дезодорирующий катализатор"]
["Защитные устройства","Компонент","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Стандартные аксессуары","Пульт дистанционного управления","","","","1"]
["","Держатель пульта дистанционного управления","","","","1"]
["","Электростатический HEPA-фильтр","","","","1"]
["","Дезодорирующий фильтр","","","","1"]
["","Руководство по эксплуатации","","","","1"]
["Шнур питания","м","","","","1.8"]
["Power supply","Фаза","","","","1~"]
["","Частота","","","Гц","50/60"]
["","Напряжение","","","V","220-240/220-230"]
["Рабочий ток","Режим очистки воздуха","","Turbo","A","0.32"]
["","","","Средний уровень","A","0.14"]
["","","","Низк.","A","0.10"]
["","","","Бесшумный","A","0.08"]
["Примечания","","","","","(1) - Обслуживаемая площадь помещения подходит для работы блока при максимальной скорости вентилятора (HH). Обслуживаемая площадь помещения — это часть, в которой может быть удалено определенное количество частиц пыли за 30 минут. (JEM 1467)"]
["","","","","","(2) - Преобразовано в стандарты NRCC на основе результатов испытаний в соответствии с JEM1467."]
["","","","","","(3) - Преобразовано в стандарты CADR на основе результатов испытаний в соответствии с JEM1467."]
["","","","","","(4) - Уровни звукового давления в процессе работы представляют собой средние значения, измеряемые на расстоянии 1 м от передней, левой, правой и верхней стороны блока. (Эти значения равны значению в безэховой камере)"]
["","","","","","(5) - Электростатический HEPA-фильтр установлен в блоке."]
["","","","","","(6) - Другие функции: Активная функция формирования плазмы. Функция автоматического перезапуска."]